******

2nd Floor Malong Building, Capitol Compound

Lingayen, Pangasinan

Tel. No. (075) 632-7840

Website@biddingandawards.pangasinan gov.ph, E-mail address: bacpangasinan@yahoo.com

**INVITATION TO BID**

**for**

**Supply and Delivery of 317 sets Hot-Dip Galvanized Street Light Pole and Solar Lights (40 Watts) and 280 sets Hot-Dip Galvanized Street Light Pole and Solar Lights (100 Watts) at Provincial Engineering Office, Lingayen, Pangasinan**

Project Identification No.: PANG-2024-01-0014-G

1. The **Provincial Government of Pangasinan**, through the **Construction, Repair & Maintenance of Various Roads and Bridges (PR#2024-01-0027)** intends to apply the sum of **One Hundred Million Pesos (P100,000,000.00)** being the Approved Budget for the Contract (ABC) to payments under the contract for **Supply and Delivery of 317 sets Hot-Dip Galvanized Street Light Pole and Solar Lights (40 Watts) and 280 sets Hot-Dip Galvanized Street Light Pole and Solar Lights (100 Watts)at Provincial Engineering Office, Lingayen, Pangasinan**.

Specifications:

**317 sets Hot-Dip Galvanized Street Light Pole and Solar Lights (40 Watts)**

***Hot Dip Galvanized Street Light Pole***

Pole Height: 6 meters

Materials: Q235, Stainless Steel

Surface Treatment: Hot Dip Galvanized

Top Diameter Range: 76mm

Bottom Diameter Range: 132mm

Pole Thickness 3mm

Base Plate Size: 250 x 250 x T12

Arm: No Arm

Quantity in 40Hg: 480 sets

Surface Treatment: Hot Dip Galvanized (inner and outside) and outdoor anti

 corrosion powder spraying

Joint of Poles: Insert Mode, Innerflange mode, face to face joint mode

Design of Pole: Against eq of 8 grade

Wind Speed: 160kph

Minimum Yield Strength: 355mpa

Minimum Ultimate Yield Strength:490mpa

Maximum Ultimate Yield Strength:620mpa

Warranty: 5 years

 Lifespan: more than 20 years

 Raw Materials Test Cutting Molding

 or Bending Welding (Longitudinal)

 Production Process: Dimension Verify Flange Welding Hole Drilling Calibration

 Debur Galvanization Powder Coating Painting

 Recalibration Thread Packages

***Solar Lights (40 Watts)***

 40W Led Solar Streetlight

 Lumens: 3800LM

 Solar Panel: 18V 35Watts Mono Crystalline

 Battery: Life PO4 177.66 WH

 Color Temperature: 4000K RA>70

 LED Source: Bridgelux 3030

 Working Time: 10-12 hours/day Full Power

 Charging Time: 6-8 hours

 Dimension: 905\*x150\*x435mm

 Frame: Aluminum Alloy

 IP Rating/IK Class: IP66/1K10

 Warranty: 3 years

**280 sets Hot-Dip Galvanized Street Light Pole and Solar Lights (100 Watts)**

***Hot Dip Galvanized Street Light Pole***

Pole Height: 8 meters

Materials: Q235, Stainless Steel

Surface Treatment: Hot Dip Galvanized

Top Diameter Range: 76mm

Bottom Diameter Range: 132mm

Pole Thickness 3mm

Base Plate Size: 250 x 250 x T12

Arm: No Arm

Quantity in 40Hg: 480 sets

Surface Treatment: Hot Dip Galvanized (inner and outside) and outdoor anti

 corrosion powder spraying

Joint of Poles: Insert Mode, Innerflange mode, face to face joint mode

Design of Pole: Against eq of 8 grade

Wind Speed: 160kph

Minimum Yield Strength: 355mpa

Minimum Ultimate Yield Strength:490mpa

Maximum Ultimate Yield Strength:620mpa

Warranty: 5 years

 Lifespan: more than 20 years

 Raw Materials Test Cutting Molding

 or Bending Welding (Longitudinal)

 Production Process: Dimension Verify Flange Welding Hole Drilling Calibration

 Debur Galvanization Powder Coating Painting

 Recalibration Thread Packages

***Solar Lights (100 Watts)***

 100W Led Solar Streetlight

 Lumens: 10,000

 Solar Panel: Mono Crystalline 130W

 Battery: Life PO4 12.8V 48AH

 Color Temperature: 4000K RA>70

 LED Source: Bridgelux 3030

 Working Time: 12 hours/day Full Power

 Charging Time: 6-8 hours

 Dimension: 1863x385x108mm

 Frame: Aluminum Alloy

 IP Rating/IK Class: IP66/1K10

 Warranty: 3 years

Bids received in excess of the ABC shall be automatically rejected at bid opening.

1. The **Provincial Government of Pangasinan** now invites bids for **Supply and Delivery of Hot-Dip Galvanized Street Light Pole and** **Solar Lights**. Delivery of the Goods is required Seven (7) Calendar Days. Bidders should have completed from the date of submission and receipt of bids, a contract similar to the project. The description of an eligible bidder is contained in the Bidding Documents, particularly, in Section II. Instruction to Bidders.
2. Bidding will be conducted through open competitive bidding procedures using a non-discretionary “pass/fail” criterion as specified in the 2016 Revised Implementing Rules and Regulation (IRR) of Republic Act (RA) 9184), otherwise known as the “Government Procurement Reform Act”

Bidding is restricted to Filipino citizen/sole proprietorships, partnerships, or organizations with at least sixty percent (60% interest or outstanding capital stock belonging to citizens of the Philippines, and to citizens or organizations of a country the laws or regulations of which grant similar rights or privileges to Filipino citizens, pursuant to RA 5183.

1. Interested bidders may obtain further information from **Provincial Government of Pangasinan** and inspect the Bidding Documents at the address given below during **January 11, 2024 – January 30, 2024; 8:00 am to 5:00pm and January 31, 2024; 8:00 am to 10:00am**.
2. A complete set of Bidding Documents may be acquired by interested Bidders **January 11, 2024 – January 30, 2024; 8:00 am to 5:00pm and January 31, 2024; 8:00 am to 10:00am at the BAC Office, 2nd Floor Malong Building, Lingayen, Pangasinan** and upon payment of the applicable fee for the Bidding Documents, pursuant to the latest Guidelines issued by the GPPB, in the amount of **Fifty Thousand Pesos (P50,000.00)**.

It may also be downloaded free of charge from the website of the Philippine Government Electronic Procurement System (PhilGEPS) and the website of the Procuring Entity, provided that Bidders shall pay the applicable fee for the Bidding Documents not later than the submission of their bids.

1. The **Provincial Government of Pangasinan** will hold a **Pre-Bid Conference** on **January 19, 2024; 2:00 pm** at **Conference Room, 2nd Floor Malong Building, Capitol Compound, Lingayen, Pangasinan**, which shall be open to prospective bidders.
2. Bids must be duly received by the BAC Secretariat at the address below on or before **January 31, 2024; 10:00am**. All bids must be accompanied by a bid security in any of the acceptable forms and in the amount stated in ITB Clause 18.

Bid opening shall be on **January 31, 2024; 10:00am** at **Conference Room, 2nd Floor, Malong Building, capitol Compound, Lingayen, Pangasinan**. Bids will be opened in the presence of the bidders’ representatives who choose to attend at the address below. Late bids shall not be accepted.

1. The **Provincial Government of Pangasinan** reserves the right to reject any and all bids, declare a failure of bidding, or not award the contract at any time prior to contract award in accordance with Section 41 of RA 9184 and its IRR, without thereby incurring any liability to the affected bidder or bidders.
2. For further information, please refer to:

**MELICIO F. PATAGUE II**

Provincial Administrator

BAC Chairman

Provincial Administrator

Capitol Building, Capitol Compound

Lingayen, Pangasinan

**MARLON C. OPERAÑA**

Provincial Accountant

BAC Technical Working Group

Provincial Accountant

Finance Building, Capitol Compound

Lingayen, Pangasinan

**ROWENA V. IGNACIO**

OIC – Provincial Planning & Dev’t Office

BAC Secretariat

BAC Office

2nd Floor Malong Building, Capitol Compound

Lingayen, Pangasinan

075 6327840

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**MELICIO F. PATAGUE II**

Provincial Administrator

BAC Chairman